|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OSPI Logo  **2019-2020** |  | |  | **PART I** | |
|  | **State Price Quote Specification**  **TYPE C60—BID AS 48 PASSENGER,**  **DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift buses for 35–60 capacity.** | | | Vendor: RWC Group |
|  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  | | | |  | |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | |
| Seating Capacity | 48 passenger based upon an average center-to-center seat spacing of at least 27.5”. | | | Capacity w/o lift 48 | | |
| Capacity w/lift 36+1 | | |
| Alternator | 240 amp minimum. Lift-equipped or air-conditioned. Manufacturer recommended capacity. | ***Diesel*** | ***Gas*** | | | ***Propane*** |
| Mfr. Leece-Neville | Mfr. Leece-Neville | | | Mfr. Leece-Neville |
| Max. amps output w/o lift or A.C. 240 | Max. amps output w/o lift or A.C. 240 | | | Max. amps output w/o lift or A.C. 240 |
| Max. amps output w/lift or A.C. 325 | Max. amps output w/lift or A.C. 320 | | | Max. amps output w/lift or A.C. 320 |
| Auxiliary Fans | 2 fans, 6” maximum, mounted to right and left windshield and service door. | | | Mfr. Bergstrom | | |
| Axle—Front | 8,000 lb. minimum. | ***Diesel*** | ***Gas*** | | | ***Propane*** |
| Mfr. Meritor/Dana | Mfr. Meritor/Dana | | | Mfr. Meritor/Dana |
| Capacity 8000 | Capacity 8000 | | | Capacity 10000 |
| Axle—Rear | 17,500 lb. minimum. | ***Diesel*** | ***Gas*** | | | ***Propane*** |
| Mfr. Dana Spicer | Mfr. Dana Spicer | | | Mfr. Dana Spicer |
| Capacity 19800 | Capacity 19800 | | | Capacity 19800 |
| Axle Oil Seals | Front and rear oil bath. | ***Diesel*** | ***Gas*** | | | ***Propane*** |
| Mfr. Stemco Voyager | Mfr. Stemco Voyager | | | Mfr. Stemco Voyager |
| Axle Ratio | Must comply with power and grade-ability formula. Refer to Washington State School Bus Specifications Manual. | ***Diesel*** | ***Gas*** | | | ***Propane*** |
| Mfr. Dana Spicer | Mfr. Dana Spicer | | | Mfr. Dana Spicer |
| Model no. 5.57 | Model no. 5.86 | | | Model no. 5.57 |
| Back-up Lights | All required backup lights to be LED (Light Emitting Diode). Refer to Washington State School Bus Specification’s Manual. | | | Round:  Diameter 7 inch  Other:  Square inches | | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification**  **TYPE C60—BID AS 48 PASSENGER,**  **DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift buses for 35–60 capacity.** | Vendor: RWC Group |
|  | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | |  | | | | | | |  | | | | | |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | | | | | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | | | | | |
|  |  | | | ***Diesel*** | | | ***Gas*** | | | | ***Propane*** | | | |
| Battery(ies) | 1200 CCA 12 volt minimum to be mounted in body battery compartment w/o lift. | | | Size/group w/o lift 31  CCA 1900 | | | Size/group w/o lift 31  CCA 1900 | | | | Size/group w/o lift 31  CCA 1900 | | | |
| 1400 CCA 12 volt minimum to be mounted in body battery compartment w/lift. | | | Size/group w/lift 31  CCA 1900 | | | Size/group w/lift 31  CCA 1900 | | | | Size/group w/lift 31  CCA 1900 | | | |
| Battery Compartment | Battery storage tray must be large enough to accommodate batteries as specified in chassis section. | | | | | | | Swing out | | | | Roll out | | |
| Brakes | Hydraulic disc. Refer to Washington State School Bus Specifications Manual. | | | | | | | Size Front 70mm Rear 70mm | | | | | | |
| Door, Service | Power operated. | | | | | | | Air  Electric  Other | | | | Folding  Split, Outward opening  Other | | |
| Engine | Diesel and Propane—180 H.P. minimum.  Gas—210 H.P. minimum. | | ***Diesel*** | | | ***Gas*** | | | | ***Propane*** | | | | |
| Engine mfr. Cummins | | | Engine mfr. PSI | | | | Engine mfr. PSI | | | | |
| Model or liters B6.7 | | | Model or liters 8.8L | | | | Model or liters 8.8L | | | | |
| Net torque 520 @ 1600 R.P.M | | | Net torque 548 @ 1800 R.P.M | | | | Net torque 565 @ 1600 R.P.M | | | | |
| Net H.P. 200 @ 2400 R.P.M | | | Net H.P. 265 @ 2600 R.P.M | | | | Net H.P. 270 @ 2600 R.P.M | | | | |
| Engine Heater | Engine manufacturer’s recommended in-block heater. | | | | | | | Watts 750 | | | | | | Volts 120 |
| Mfr. Phillips | | | | | | |
| Engine Temperature | To be controlled electronically, by fan clutch/drive, or shutters. | | | | | | | Mfr. Borg Warner | | | | | | Electronic |
| Fan clutch | | | | | | Shutters |
| Fuel Tank | Diesel and Gas—60 gallon minimum.  Propane—largest available. | | | | ***Diesel*** | | | ***Gas*** | | | | | ***Propane*** | |
| Capacity 65 | | | Capacity 60 | | | | | Capacity 46.25 | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification**  **TYPE C60—BID AS 48 PASSENGER,**  **DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift buses for 35–60 capacity.** | Vendor: RWC Group |
|  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | |  | |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | |
| Heaters | Minimum of 210,000 BTU total. Shutoff valves at engine for all heaters. Two-speed motors. Must include recirculating pump. | Left-front B.T.U. 90,000 | | Right-front B.T.U. 50,000 |
| Center B.T.U. 50,000 | | Rear B.T.U. 50,000 |
| Total B.T.U. 240,000 | |  |
| Hood | Tilt. | Fiberglass | | Metal |
| Lights | LED (Light Emitting Diode). Includes Clearance Lights, Stop Lights–7”, Tail Lights, Turn Signals, Eight-Light System, and Dome-Light System. | Check if as specified  If not, explain | | |
| P.A. System | AM/FM/PA radio with 2 interior and 1 exterior speakers. | Mfr. Panasonic | | |
| Model No. CRCM120UA | | |
| Seat Spacing | To permit specified passenger capacity based on an average center-to-center seat spacing of at least 27.5”. | Inside measurement from rear of stepwell to  appropriate point at rear of passenger  seating area: w/o lift 270.9 w/lift 270.9 | | |
| Mfg.’s C/C seat measurement of vehicle  (inches): w/o lift 31.12 w/lift 31.35 | | |
| Steering Wheel | Tilt and telescoping column. | Check if as specified | | |
| Step Tread | Studded or pebbled top tread covering. | Mfr. Koroseal | | |
| Tires | 6 first quality, radial ply. No low profile tires. | Mfr. Hankook | | |
| Size 22.5 | | |
| Load range 8.25 | | |
| Toolbox | Exterior, manufacturer standard. | Size (cubic feet) 2.82 | | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification**  **TYPE C60—BID AS 48 PASSENGER,**  **DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift buses for 35–60 capacity.** | Vendor: RWC Group |
|  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | |  | | | | | | |  | |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | | | | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | | |
| Transmission | Diesel and Propane: Automatic—Allison, PTS 2500 or equal.  Gas: Automatic—manufacturer’s standard compatible with H.P. and torque rating of engine bid. | | | ***Diesel*** | ***Gas*** | | | | | ***Propane*** |
| Mfr. Allison | Mfr. Allison | | | | | Mfr. Allison |
| Model no. 2550 6 spd | Model no. 2550 6 spd | | | | | Model no. 2550 6 spd |
| Net input 520 | Net input 520 | | | | | Net input 520 |
| Net input H.P. 200 | Net input H.P. 200 | | | | | Net input H.P. 200 |
| Two-way Communications | 45-watt, VHF, mil. spec. | | | | | Mfr. ICOM | | | | |
| Model No. F-5011 | | | | |
| Wheels | 6 to be compatible with tire size. | | | | | Size 22.5 | | | | |
| Rim width 8.25 | | | | |
|  | | | **SPECIAL NEEDS REQUIREMENTS—CHASSIS AND BODY** | | | | |  | | |
| Wheelchair  Lift—Installed | Must meet state specification. Platform shall be a minimum of 32” x 52”. | | | | | Mfr. Braun Gen2 | | | | |
| Model No. NL919FIB | | | | |
| Wheelchair/ Occupant Tie-down System—Installed | Must meet state specification. | | | | | Mfr. Q-Straint | | | | |
| Model No. Q-8100-A1-SC | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification**  **TYPE C60—BID AS 48 PASSENGER,**  **DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift buses for 35–60 capacity.** | Vendor: RWC Group |
|  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | |  |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | |
|  | **ADDITIONAL REQUIREMENTS—CHASSIS AND BODY** | |  |
| Line Setting Ticket | Legible copy of manufacturer’s Line Setting Ticket will be delivered with each vendor’s packet at the time of delivery of the bus. | Check if as specified | |
| Owner’s/Operator’s Handbook | One copy of the chassis manufacturer’s owner’s/operator’s handbook or manual will be furnished with each bus at time of delivery. | Check if as specified | |
| Repair Manuals | A complete set of chassis, engine, transmission, and body repair manuals, including wiring diagram for all components, will be made available at time of delivery, with instructions available on accessing repair materials. | Check if as specified | |
| Service and Cleaning | Cleaning and service by vendor prior to delivery will include:   * Chassis lubrication. * Check fluid levels: verify all are at recommended full levels. * Cooling system protected at -20°F. * Interior and exterior will be clean (including glass). * All systems (electric, air, hydraulic, mechanical and manual) be inspected to ensure proper operation at time of delivery. * All components and accessories will be installed and operational at time of delivery. | Check if as specified | |
| Warranty | A complete copy of all warranty agreements will be furnished at time of delivery. | Check if as specified | |

|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo  **2019-2020** | STUDENT TRANSPORTATION  Old Capitol Building  PO BOX 47200  Olympia, WA 98504-7200  (360) 725-6120 TTY (360) 664-3631  **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION**  **TYPE C60—BID AS 48 PASSENGER (DIESEL)** | | |
|  | |  | |
| VENDOR’S COMPANY NAME  RWC Group | | REPRESENTATIVE’S NAME  Tom Hartman | TELEPHONE NUMBER  602-377-4401 |
| ADDRESS  600 North 75th Avenue  Phoenix, AZ 85043 | | Estimated delivery date to school district from time purchase order is received: 180 Days ARO  Firm where engine and chassis can be  serviced or repaired and parts obtained: Any IC or International Dealer  Firm where body can be serviced or repaired and parts obtained: RWC Group (4 locations in WA) | |
|  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **BODY** | | | | |
| MAKE  IC Corporation | | Warranty: Years 5  Miles Unlimit  Seat color: Gray  Floor color: Black | Inside measurement from rear of stepwell to appropriate point at  rear of passenger seating area:  w/o lift 270.9 w/lift 270.9 | Equipped seating capacity:  w/o lift 48 w/lift 36+1  Overall vehicle length (inches):  w/o lift 384.9 w/lift 384.9 |
| MODEL  PB105 | YEAR  2021 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CHASSIS** | | | **ENGINE** | | |
| MAKE  IC Corporation | | Warranty: Years 5  Miles Unlimit | MANUFACTURER  Cummins | | Torque: 520 @ 1600 RPM  H.P.: 200 @ 2400 RPM |
| MODEL  PB105 | YEAR  2021 | Wheel base: 218 | MODEL  B6.7 | YEAR  2021 | C.I.D. or Liters: 409  Fuel type: Diesel |
| **TRANSMISSION** | | | Warranty: Years 5  Miles 100,000  Number of cylinders: 6  Inline X V-type | | Battery type/grp: 31 31  Number batteries: 2 2  Total CCA: 1900 1900 |
| MANUFACTURER  Allison | | Speeds forward: 6 |
| MODEL  2550/2500 | | Warranty: Years 7  Miles Unlimit |

|  |  |
| --- | --- |
| **QUOTED PRICE** | |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).  Diesel Bid—w/o lift $ 92,369 Diesel Bid—w/lift $ 96,611 | |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo  **2019-2020** | STUDENT TRANSPORTATION  Old Capitol Building  PO BOX 47200  Olympia, WA 98504-7200  (360) 725-6120 TTY (360) 664-3631  **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION**  **TYPE C60—BID AS 48 PASSENGER (GAS)** | | |
|  | |  | |
| VENDOR’S COMPANY NAME  RWC Group | | REPRESENTATIVE’S NAME  Tom Hartman | TELEPHONE NUMBER  602-377-4401 |
| ADDRESS  600 North 75th Avenue  Phoenix, AZ 85043 | | Estimated delivery date to school district from time purchase order is received: 180 Days ARO  Firm where engine and chassis can be  serviced or repaired and parts obtained: Any IC or International Dealer  Firm where body can be serviced or repaired and parts obtained: RWC Group | |
|  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **BODY** | | | | |
| MAKE  IC Corporation | | Warranty: Years 5  Miles Unlimit  Seat color: Gray  Floor color: Black | Inside measurement from rear of stepwell to appropriate point at  rear of passenger seating area:  w/o lift 261.9 w/lift 261.9 | Equipped seating capacity:  w/o lift 48 w/lift 36+1  Overall vehicle length (inches):  w/o lift 375.9 w/lift 375.9 |
| MODEL  PB105 | YEAR  2021 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CHASSIS** | | | **ENGINE** | | |
| MAKE  IC Corporation | | Warranty: Years 5  Miles Unlimit | MANUFACTURER  PSI | | Torque: 548 @ 1800 RPM  H.P.: 265 @ 2600 RPM |
| MODEL  PB105 | YEAR  2021 | Wheel base: 218 | MODEL  8.8L | YEAR  2021 | C.I.D. or Liters: 8.8L  Fuel type: Gas |
| **TRANSMISSION** | | | Warranty: Years 5  Miles Unlimited  Number of cylinders: 8  Inline       V-type X | | Battery type/grp: 31 31  Number batteries: 2 2  Total CCA: 1900 1900 |
| MANUFACTURER  Allison | | Speeds forward: 6 |
| MODEL  2550/2500 | | Warranty: Years 7  Miles Unlimit |

|  |  |
| --- | --- |
| **QUOTED PRICE** | |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).  Gas Bid—w/o lift $ 89,894 Gas Bid—w/lift $ 94,136 | |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo  **2019-2020** | STUDENT TRANSPORTATION  Old Capitol Building  PO BOX 47200  Olympia, WA 98504-7200  (360) 725-6120 TTY (360) 664-3631  **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION**  **TYPE C60—BID AS 48 PASSENGER (PROPANE)** | | |
|  | |  | |
| VENDOR’S COMPANY NAME  RWC Group | | REPRESENTATIVE’S NAME  Tom Hartman | TELEPHONE NUMBER  602-377-4401 |
| ADDRESS  600 North 75th Avenue  Phoenix, AZ 85043 | | Estimated delivery date to school district from time purchase order is received: 180 Days ARO  Firm where engine and chassis can be  serviced or repaired and parts obtained: Any IC or International Dealer  Firm where body can be serviced or repaired and parts obtained: RWC Group | |
|  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **BODY** | | | | |
| MAKE  IC Corporation | | Warranty: Years 5  Miles Unlimit  Seat color: Gray  Floor color: Black | Inside measurement from rear of stepwell to appropriate point at  rear of passenger seating area:  w/o lift 270.9 w/lift 270.9 | Equipped seating capacity:  w/o lift 48 w/lift 36+1  Overall vehicle length (inches):  w/o lift 384.9 w/lift 384.9 |
| MODEL  PB105 | YEAR  2021 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CHASSIS** | | | **ENGINE** | | |
| MAKE  IC Corporation | | Warranty: Years 5  Miles Unlimit | MANUFACTURER  PSI | | Torque: 565 @ 1600 RPM  H.P.: 270 @ 2600 RPM |
| MODEL  PB105 | YEAR  2021 | Wheel base: 218 | MODEL  8.8L | YEAR  2021 | C.I.D. or Liters: 8.8L  Fuel type: Propane |
| **TRANSMISSION** | | | Warranty: Years 5  Miles Unlimited  Number of cylinders: 8  Inline       V-type X | | Battery type/grp: 31 31  Number batteries: 2 2  Total CCA: 1900 1900 |
| MANUFACTURER  Allison | | Speeds forward: 6 |
| MODEL  2550/2500 | | Warranty: Years 7  Miles Unlimit |

|  |  |
| --- | --- |
| **QUOTED PRICE** | |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).  Propane Bid—w/o lift $ 102,758 Propane Bid—w/lift $ 106,970 | |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

PART II

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification**  **DISTRICT-SUPPORTED OPTIONS**  **C60**  **C77**  **D60**  **D84**  **Use this document to bid both non-lift and lift buses.** | Vendor: RWC Group |
|  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | |  | |
| **ITEM** | Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the district cost. | | |
| Activity Securement Seating | 2-passenger position seats with lap-shoulder belts in all passenger positions. | Passenger Capacity 32 | | |
| Cost $ 17,216 | | |
| Air Conditioning | To cool passenger compartment as required in the Washington State School Bus Specifications manual. | Mfr. TransAir 120k | | |
| Cost $ 9,513 | | |
| Alternate Fuel | Must comply with power and gradeability formula. Refer to Washington State School Bus Specifications manual. Must comply with all of the requirements of FMVSS No. 305. | Mfr. N/A | | |
| CNG | CNG Cost $ | | |
| Electric | Electric Cost $ | | |
| Alternator | Available options. | Cost $ 882 Capacity 325 | | |
| Cost $       Capacity | | |
| Cost $       Capacity | | |
| Anti-spray Device | Rubber fender extenders. | Type C: Cost $ Included | | |
| Type D: Cost $ 272 | | |
| Back-up Alarm | Must meet state specification. | Mfr. Ecco SA-917-87 | | |
| Cost $ 123 | | |
| Brakes | 4-wheel hydraulic disk brake. | Cost $ Standard | | Deduct $ N/A |
| Brakes | Air, Drum or Disc. Refer to Washington State School Bus Specifications manual. | Disc Cost $ 3,227-Air | | Disc Deduct $ N/A |
| Drum Cost $ Standard | | Drum Deduct $ N/A |
| Color | Exterior white roof. | Cost $ 776 | | |
| Door Locks | Vandal lock system on all exterior doors. | Cost $ 718 | | |
| Driver’s Seat | Suspension type, 6-way adjustable, with lumbar adjustment. Cloth panel covers. | ***Non-Air*** | | ***Air*** |
| Mfr. Magnum | | Mfr. National |
| Cost $ 225 | | Cost $ 397 |
| Fire Suppression System | Jomarr VT-6-E-NAF, or equal engine compartment fire suppression system of appropriate size to be installed according to manufacturer recommendation. | Mfr. Fogmaker | | |
| Cost $ 4,580 | | |

PART II (cont.)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification**  **DISTRICT-SUPPORTED OPTIONS**  **C60  C77  D60  D84**  **Use this document to bid both non-lift and lift buses.** | Vendor: RWC Group |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  | | |
| **ITEM** | Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the district cost. | |
| Floor Color | Nonstandard color. | | Cost $ 419 | |
| Fuel Tank | Larger fuel capacity (CNG only). | | Size: N/A | Cost $ |
| Fuel Tank | Larger fuel capacity (Diesel only). | | Size: N/A | Cost $ |
| Fuel Tank | Larger fuel capacity (Propane only). | | Size: N/A | Cost $ |
| Headlights | Halogen. | | Cost $ Included | |
| Headlights | L.E.D. | | Cost $ N/A | |
| Heater (Auxiliary water) | Auxiliary fuel-fired heating systems. Refer to Washington State School Bus Specifications Manual, page 27. | | Brand: Webasto Model: Scholastic | |
| Cost $ 3,171 | |
| Noise Reduction | Exceeding minimum specifications. | | Driver compartment Cost $ 159 | |
| Engine compartment Cost $ 333 | |
| Full acoustical headliner Cost $ Included | |
| Retarder | Manufacturer’s standard. | | Driveline  Cost $ | |
| Exhaust  Cost $ 184 | |
| Transmission  Cost $ | |
| Seat Belt Ready Seat | 3-passenger position seat with securement belts. | | Cost $ 758 | |
| Seating System | Identical, non-lift bus with lap-shoulder seat belt system installed in all positions. | | 2 by 2 Cost $ 8,886 | |
| Capacity 32 | |
| 3 by 2 Cost $ N/A | |
| Capacity N/A | |
| 3 by 3 Cost $ 9,834 | |
| Capacity 48 | |

PART II (cont.)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification**  **DISTRICT-SUPPORTED OPTIONS**  **C60  C77  D60  D84**  **Use this document to bid both non-lift and lift buses.** | Vendor: RWC Group |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  | | | |
| **ITEM** | Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the district cost. | | |
| Storage Compartments | Largest available for unit bid. | | Left-side 16.5 cubic feet. | | |
| Cost $ 1,116 | | |
| Right-side 16.5 cubic feet. | | |
| Cost $ 1,116 | | |
| Push-thru N/A cubic feet. | | |
| Cost $ N/A | | |
| Strobe Light | Exterior roof mounted white strobe light. | | Mfr. ECCO | | |
| Model No. 6550 | | |
| Cost $ 217 | | |
| Student Protection System—Installed | Electronic system to insure driver post-trip inspection of passenger compartment. | | Mfr. IC | | |
| Model No. Leave no student behind | | |
| Cost $ Included | | |
| Suspension | Air ride (Air brake system only). | | ***Front*** | ***Rear*** | |
| Cost $ N/A | Cost $ 1,233 | |
| Toolbox | Interior, manufacturer standard. | | Cost $ 50 | Deduct $ 62 | |
| Traction Device | Automatic chains. | | Mfr. On Spot | | |
| Cost $ 3,514 | | |
| Traction Device | Sanders. | | Capacity 10 Gallon | | |
| Cost $ 3,500 | | |
| Transmission | Automatic—Allison, PTS 3000 or equal. | | Mfr. Allison | | |
| Model No. 3000 | | |
| Cost $ 5,100 | | |
| Vehicle Securement System | Must meet state specification. | | Mfr. SBS | | Cost $ 852 |

PART II (cont.)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification**  **DISTRICT-SUPPORTED OPTIONS**  **C60  C77  D60  D84**  **Use this document to bid both non-lift and lift buses.** | Vendor: RWC Group |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  | | |
| **ITEM** | Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the district cost. | |
| Video Camera Systems—Installed | Digital audio/video system for monitoring the passenger compartment with more than two cameras. | | Mfr. Seon | |
| Model No. TH4 | |
| Cost $ 2,664 How many cameras 3 | |
| Video Camera Systems—Stop Sign Camera—Installed | Must meet state specification. | | ***Stand Alone System*** | ***Added to Interior System*** |
| Mfr. Seon | Mfr. Seon |
| Model No. TH4 | Model No. TH4 |
| Cost $ 2,307 | Cost $ 795 |
| How many cameras 1 | How many cameras 1 |
| Warning Light Monitor | 16 light monitoring system. | | ***Incandescent*** | ***LED Lights*** |
| Cost $ 191 | Cost $ 217 |
| Additional Wheelchair/Occupant Tie-down System—Installed | Must meet state specification. | | Mfr. Q Straint | |
| Model No. Q-8100-A1-SC | |
| Cost per station $ 1,115 | |
| Windows | Laminated passenger-compartment side or rear glass. | | Side Cost $ 972 | |
| Rear Cost $ 147 | |
| Both Cost $ 1,119 | |
| Windows | Tinted. | | Cost $ 524 | |
| Windows | Thermal pane, left of driver and service door. | | Cost $ 555 | |