|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo**2018-19** |  |  | **PART I** |
|  | **State Price Quote Specification****TYPE A— DIESEL, GAS & PROPANE****Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor:  Northwest Bus Sales, Inc  Mfr.:   Starcraft     |
|  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the state cost. |
| Seating Capacity | Maximum passenger capacity based upon an average center-to-center seat spacing of at least 27.5” with a lap-shoulder belt for each seating position. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Capacity w/o lift   26   | Capacity w/o lift    21   | Capacity w/o lift   n/a     |
| Capacity w/lift 18 +1WC   | Capacity w/lift 12 +1WC | Capacity w/lift n/a  |
| Alternator | 145 amp minimum. Lift-equipped or air-conditioned. Manufacturer recommended capacity. | Mfr.   GM / Diesel: Ford   |
| Amps output w/o lift or A.C.  Gas: 145/ Diesel: 150   |
| Amps output w/lift or A.C.   Gas: 145/ Diesel: 150  |
| Auxiliary Automatic Transmission Cooler | 10,000 lb. Hayden or equal. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Mfr.   GM     | Mfr.    Ford    | Mfr.    n/a    |
| Lbs. rating   10,000     | Lbs. rating 10,000    | Lbs. rating   n/a      |
| Axle—Front | Manufacturer’s recommendation. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Mfr.   GM     | Mfr.    Ford    | Mfr.   n/a       |
| Capacity  4,300      | Lbs. rating   4,130     | Lbs. rating    n/a      |
|  |  | Indepen. suspens. X | Indepen. suspens. X | Indepen. suspens.  |
| Axle—Rear | Manufacturer’s recommendation. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Mfr.  GM      | Mfr.    Ford    | Mfr.     n/a     |
| Capacity   8,000     | Capacity   6,230     | Capacity    n/a      |
| Axle Ratio | Must comply with power and gradeability formula. Refer to Washington State School Bus Specifications Manual. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Ratio    3.73    | Ratio   3.73     | Ratio    n/a      |
| Back-up Lights | All required backup lights to be LED (Light Emitting Diode). Refer to Washington State School Bus Specification’s Manual. | Round: X Diameter   4”6    Other: ☐ Square inches        |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification****TYPE A— DIESEL, GAS & PROPANE****Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor:Northwest Bus Sales, Inc Mfr.:  Starcraft       |
|  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the state cost. |
| Battery(ies) | 535 CCA 12 volt minimum for gas and propane w/o lift.1070 CCA 12 volt minimum for diesel or any bus w/lift. | ***Gas/Propane w/o lift*** | ***Diesel or any bus w/lift*** |
| CCA   700     | CCA   n/a       |
| Brakes | Hydraulic: Drum or Disc. Refer to Washington State School Bus Specifications Manual. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Front Disc X | Front Disc X | Front Disc  |
|  Drum ☐ |  Drum ☐ |  Drum ☐ |
| Rear Disc X | Rear Disc X | Rear Disc  |
|  Drum ☐ |  Drum ☐ |  Drum ☐ |
| Drum Size        | Drum Size        | Drum Size        |
| Doors, Service | Power operated. | ☐ Air ☐ Folding X Electric☐ Split, Outward Opening ☐ Other        |
| Engine | Gas and Propane—3.7 liters minimum.Diesel—130 H.P. minimum. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Engine mfr.   GM    | Engine mfr.   Ford     | Engine mfr.     n/a     |
| Liters   6.0     | H.P.  185      | Liters    n/a      |
| Engine Heater | Diesel only—engine manufacturer’s recommended in-block heater. | Watts   400     | Volts   110     |
| Mfr.  Ford      |
| Fuel Tank | Gas and Diesel—25 gallon minimum.Propane—largest available. | ***Gas/Diesel*** | ***Propane*** |
| Capacity   25     | Capacity   n/a    |
| Hand Throttle | Diesel only—locking type, electronic, or immediate acting electric fast idle. |  ☐ Vernier |  ☐ Electric |
|  ☐ T type |  X Electronic |
| Heaters | Front—manufacturer’s standard. Rear—40,000 B.T.U. minimum. | Rear B.T.U. w/o lift   65,000    Rear B.T.U. w/lift   65,000     |
| Lights | LED (Light Emitting Diode). Includes Clearance Lights, Stop Lights–7”, Tail Lights, Turn Signals, Eight-Light System, and Dome-Light System. | Check if as specified XIf not, explain   |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification****TYPE A— DIESEL, GAS & PROPANE****Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: Northwest Bus Sales, Inc  Mfr.:   Starcraft  |
|  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the state cost. |
| P.A. System | AM/FM/PA radio with 2 interior and 1 exterior speakers. | Mfr.   Jensen     |
| Model No.  BR550/ PA500      |
| Seat Spacing | To permit specified passenger capacity based on an average center-to-center seat spacing of at least 27.5”. | Inside measurement from rear of stepwell toappropriate point at rear of passenger seatingarea: w/o lift Gas: 160.185 Diesel: 170.375 w/lift Gas: 160.185 Diesel: 170.375 |
| Mfg.’s C/C seat measurement ofvehicle (inches): w/o lift    28   w/lift   28     |
| Steering Wheel | Tilt. | Check if as specified X |
| Step Tread | Studded or pebbled top tread covering. | Mfr.  Koloseal      |
| Tires | 6 first quality, radial ply.  | Mfr.   OEM     |
| Size   Gas: LT225-75R16E/ Diesel: 195/75R16     |
| Load range    E    |
| Toolbox | Exterior, manufacturer standard. | Size (cubic feet)   3.35     |
| Transmission | Automatic—manufacturer’s standard compatible with H.P. and torque rating of engine bid. | ***Gas*** | ***Diesel*** | ***Propane*** |
| Mfr.   GM     | Mfr.    Ford    | Mfr.   n/a       |
| Model no.   6L90     | Model no.  SelectShift      | Model no.    n/a      |
| Two-way Communications | 45-watt, VHF, mil. spec. | Mfr.     ICOM   |
| Model No. F5011 Series       |
| Wheels | 6 to be compatible with tire size. | Size   16     |
| Rim width   Gas: 6.5 / Diesel: 6/ Propane : 6     |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification****TYPE A— DIESEL, GAS & PROPANE****Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor:  Northwest Bus Sales, Inc  Mfr.:   Starcraft     |
|  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the state cost. |
|  | **SPECIAL NEEDS REQUIREMENTS—CHASSIS AND BODY** |  |
| WheelchairLift—Installed | Must meet state specification. Platform shall be a minimum of 32” x 52”. | Mfr.   Braun     |
| Model No.  Century NCL9191B-2      |
| Wheelchair/Occupant Tie-down System—Installed | Must meet state specification. | Mfr.  Q-Straight      |
| Model No.  Q8101 / Q8-6326-A1      |
|  | **ADDITIONAL REQUIREMENTS—CHASSIS AND BODY** |  |
| Line Setting Ticket | Legible copy of manufacturer’s Line Setting Ticket will be delivered with each vendor’s packet at the time of delivery. | Check if as specified X |
| Owner’s/Operator’s Handbook | One copy of the chassis manufacturer’s owner’s/operator’s handbook or manual will be furnished with each bus at delivery. | Check if as specified X |
| Repair Manuals | A complete set of chassis, engine, transmission, and body repair manuals, including wiring diagram for all components, will be made available at time of delivery, with instructions available on accessing repair materials. | Check if as specified X |
| Service and Cleaning | Cleaning and service by vendor prior to delivery will include:* Chassis lubrication.
* Check fluid levels: verify all are at recommended full levels.
* Cooling system protected at -20°F.
* Interior and exterior will be clean (including glass).
* All systems (electric, air, hydraulic, mechanical and manual) be inspected to ensure proper operation at time of delivery.
* All components and accessories will be installed and operational at time of delivery.
 | Check if as specified X |
| Warranty | A complete copy of all warranty agreements will be furnished at time of delivery. | Check if as specified X |

|  |  |
| --- | --- |
| OSPI Logo**2018-19** |  STUDENT TRANSPORTATION Old Capitol Building PO BOX 47200 Olympia, WA 98504-7200 (360) 725-6120 TTY (360) 664-3631 **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION** **TYPE A—DIESEL** |
|  |  |
| VENDOR’S COMPANY NAME     Northwest Bus Sales, Inc | REPRESENTATIVE’S NAME    Rob Goolsby  | TELEPHONE NUMBER     800-231-7099 |
| ADDRESS     33207 Pacific Hwy S Federal, WA 98003 | Estimated delivery date to school district from time purchase order is received:  150-180 days     Firm where engine and chassis can be serviced or repaired and parts obtained:  Any Ford Dealer    Firm where body can be serviced or repaired and parts obtained:    Northwest Bus Sales, Inc    |
|  |

|  |
| --- |
| **BODY** |
| MAKE     Starcraft  | Warranty: Years  3     Miles 36,000Seat color:  Gray    Floor color:   Black    | Inside measurement from rear of stepwell to appropriate point at rear of passenger seating area: w/o lift 170,375 w/lift 170,375  | Equipped seating capacity: w/o lift   21   w/lift 12+1WCOverall vehicle length (inches): w/o lift  275,0625 w/lift  275,0625  |
| MODEL Quest      | YEAR     2019 |

|  |  |
| --- | --- |
| **CHASSIS** | **ENGINE** |
| MAKE     Ford | Warranty: Years   3    Miles 36,000 | MANUFACTURER     Ford | Torque: 350 @1500-2500  RPMH.P.:  185 @  3000 RPM |
| MODEL     Transit | YEAR    2019 | Wheel base:    156   | MODEL 3.2L PowerStroke I-5 | YEAR  2019    | Fuel type:    Diesel   |
| **TRANSMISSION** | Warranty: Years  5      Miles    60,000  Number of cylinders:   5   Inline  X     V-type       | Battery type/grp:   12V  12VNumber batteries:   2      2 Total CCA: 1,520    1,520  |
| MANUFACTURER     Ford | Speeds forward:  6    |
| MODEL     Select Shift  | Warranty: Years   3    Miles 36,000  |

|  |
| --- |
| **QUOTED PRICE** |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).Diesel Bid—w/o lift $ 58,116   Diesel Bid—w/lift $61,734    |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |
| --- | --- |
| OSPI Logo**2018-19** |  STUDENT TRANSPORTATION Old Capitol Building PO BOX 47200 Olympia, WA 98504-7200 (360) 725-6120 TTY (360) 664-3631 **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION** **TYPE A—GAS** |
|  |  |
| VENDOR’S COMPANY NAME     Northwest Bus Sales, Inc | REPRESENTATIVE’S NAME    Rob Goolsby   | TELEPHONE NUMBER     800-231-7099 |
| ADDRESS     33207 Pacific Hwy S Federal, WA 98003 | Estimated delivery date to school district from time purchase order is received:  150-180 days     Firm where engine and chassis can beserviced or repaired and parts obtained:  Any GM Dealer     Firm where body can be serviced or repaired and parts obtained:  Northwest Bus Sales, Inc       |
|  |

|  |
| --- |
| **BODY** |
| MAKE     Starcraft | Warranty: Years   3    Miles 36,000 Seat color:   Gray   Floor color:  Black     | Inside measurement from rear of stepwell to appropriate point at rear of passenger seating area: w/o lift 160,1875 w/lift 160,187  | Equipped seating capacity: w/o lift  26 w/lift 18+1WCOverall vehicle length (inches): w/o lift 266,3125  w/lift 266,3125 |
| MODEL     Quest  | YEAR     2019 |

|  |  |
| --- | --- |
| **CHASSIS** | **ENGINE** |
| MAKE  Chevrolet     | Warranty: Years   3    Miles 36,000  | MANUFACTURER  GM    | Torque: 373 @  4,400 RPMH.P.:  342   @  5,400  RPM |
| MODEL    Express 3500  | YEAR   2019  | Wheel base:  139     | MODEL    Vortec 6.0L  | YEAR  2019    | Liters:  6.0    Fuel type:  Gas     |
| **TRANSMISSION** | Warranty: Years   5     Miles  100,000    Number of cylinders:   8   Inline       V-type   X    | Battery type/grp:   12V   12V  Number batteries:   2       2  Total CCA:  1430     1430  |
| MANUFACTURER     Chevrolet | Speeds forward:   6    |
| MODEL     6L90 | Warranty: Years   5    Miles 100,000 |

|  |
| --- |
| **QUOTED PRICE** |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).Gas Bid—w/o lift $ 55,391   Gas Bid—w/lift $ 58,682    |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART II** |
|  | **State Price Quote Specification****DISTRICT-SUPPORTED OPTIONS****TYPE A****Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: Northwest Bus Sales, Inc  Mfr.:    Starcraft   |
|  |

|  |  |  |
| --- | --- | --- |
|  | **CHASSIS** |  |
| **ITEM** | Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Small A | Type A bus—10,000 lbs or under GVWR chassis. | ***Gas*** |  ***Diesel***  | ***Propane*** |
| Deduct   N/A     | Deduct   N/A     | Deduct  N/A      |
| Mfr.        | Mfr.   N/A    | Mfr.        |
| Capacity w/o lift        | Capacity w/o lift        | Capacity w/o lift        |
| Dual Wheel ☐ | Dual Wheel ☐ | Dual Wheel ☐ |
| Single Wheel ☐ | Single Wheel ☐ | Single Wheel ☐ |
| Air Conditioning | To cool passenger compartment as required in the Washington State School Bus Specifications manual. | Mfr.  Transair      |
| Cost $ 1,695       |
| Alternate Fuel | Must comply with power and gradeability formula. Refer to Washington State School Bus Specifications manual. Must comply with all of the requirements of FMVSS No. 305. | Mfr.   Icom     |
| ☐ CNG | ☐ CNG Cost $        |
| ☐ Electric | ☐ Electric Cost $        |
| Back-up Alarm | Must meet state specification. | Mfr.   Ecco     |
| Cost $ 19.88      |
| Color | Exterior white roof. | Cost $  Standard      |
| Steering Wheel | Tilt and telescoping column. | Cost $  Tilt Only - STANDARD- Non Telescoping      |
| Strobe Light | Exterior roof mounted white strobe light. | Mfr.   Sound Off Signal     |
| Model No.    3107LCC    |
| Cost $ 193       |
| Student Protection System—Installed | Electronic system to insure driver post-trip inspection of passenger compartment.  | Mfr. Child Checkmate       |
| Model No. DLRH-1       |
| Cost $ 245       |
| Toolbox | Interior, manufacturer standard. | Cost $ 162.50       | Deduct $        |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART II (cont.)** |
|  | **State Price Quote Specification****DISTRICT-SUPPORTED OPTIONS****TYPE A****Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: Northwest Bus Sales, Inc Mfr.:   Starcraft     |
|  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **ITEM** | Vendor must meet or exceed these specifications.Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**Price of items bid will establish the district cost. |
| Video Camera Systems—Installed | Digital audio/video system for monitoring the passenger compartment with more than two cameras. | Mfr.  Angel Trax      |
| Model No.   Hybrid Quest      |
| Cost $3350       How many cameras    3   |
| Video Camera Systems—Stop Sign Camera—Installed | Must meet state specification. | ***Stand Alone System*** | ***Added to Interior System*** |
| Mfr.   Angel Trax     | Mfr.   Angel Trax     |
| Model No.Hybrid Quest   | Model No. Hybrid Quest   |
| Cost $2,940   | Cost $ 3,425       |
| How many cameras  1  | How many cameras  4   |
| Warning Light Monitor | 16 light monitoring system. | ***Incandescent*** | ***LED Lights*** |
| Cost $ 525       | Cost $ 525       |
| Additional Wheelchair/Occupant Tie-down System—Installed | Must meet state specification. | Mfr. Q-Straint       |
| Model No.  Q8101 / Q8-6326-A1  |
| Cost per station $ 950       |
| Windows | Laminated passenger-compartment side or rear glass. | Side Cost $  985      |
| Rear Cost $  425      |
| Both Cost $  1410      |
| Windows | Tinted. | Cost $  STANDARD      |