|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OSPI Logo  **2018-19** |  | |  | **PART I** | |
|  | **State Price Quote Specification**  **TYPE C60—BID AS 48 PASSENGER,**  **DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift buses for 35–60 capacity.** | | | Vendor: SCHETKY NW SALES, INC. |
|  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  | | | |  | |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | |
| Seating Capacity | 48 passenger based upon an average center-to-center seat spacing of at least 27.5”. | | | Capacity w/o lift 48 | | |
| Capacity w/lift 28 W/DIESEL / 43 W/PROPANE | | |
| Alternator | 240 amp minimum. Lift-equipped or air-conditioned. Manufacturer recommended capacity. | ***Diesel*** | ***Gas*** | | | ***Propane*** |
| Mfr. LEECE-NEVILLE / DELCO REMMY | Mfr. N/A | | | Mfr. LEEC-NEVILLE / DELCO REMMY |
| Max. amps output w/o lift or A.C. 200 | Max. amps output w/o lift or A.C. N/A | | | Max. amps output w/o lift or A.C. 200 |
| Max. amps output w/lift or A.C. 240 | Max. amps output w/lift or A.C. N/A | | | Max. amps output w/lift or A.C. 240 |
| Auxiliary Fans | 2 fans, 6” maximum, mounted to right and left windshield and service door. | | | Mfr. BERGSTROM | | |
| Axle—Front | 8,000 lb. minimum. | ***Diesel*** | ***Gas*** | | | ***Propane*** |
| Mfr. DETROIT | Mfr. N/A | | | Mfr. DETROIT |
| Capacity 8,000 | Capacity N/A | | | Capacity 8,000 |
| Axle—Rear | 17,500 lb. minimum. | ***Diesel*** | ***Gas*** | | | ***Propane*** |
| Mfr. DETROIT | Mfr. N/A | | | Mfr. DETROIT |
| Capacity 17.5K | Capacity N/A | | | Capacity 17.5K |
| Axle Oil Seals | Front and rear oil bath. | ***Diesel*** | ***Gas*** | | | ***Propane*** |
| Mfr. CHICAGO RAWHIDE | Mfr. N/A | | | Mfr. CHICAGO RAWHIDE |
| Axle Ratio | Must comply with power and grade-ability formula. Refer to Washington State School Bus Specifications Manual. | ***Diesel*** | ***Gas*** | | | ***Propane*** |
| Mfr. DETROIT | Mfr. N/A | | | Mfr. DETROIT |
| Model no. 17-2 | Model no. N/A | | | Model no. 17-2 |
| Back-up Lights | All required backup lights to be LED (Light Emitting Diode). Refer to Washington State School Bus Specification’s Manual. | | | Round:  Diameter 7"  Other:  Square inches 22" | | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification**  **TYPE C60—BID AS 48 PASSENGER,**  **DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift buses for 35–60 capacity.** | Vendor: SCHETKY NW SALES, INC. |
|  | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | |  | | | | | | |  | | | | | |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | | | | | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | | | | | |
|  |  | | | ***Diesel*** | | | ***Gas*** | | | | ***Propane*** | | | |
| Battery(ies) | 1200 CCA 12 volt minimum to be mounted in body battery compartment w/o lift. | | | Size/group w/o lift 31  CCA 1500 | | | Size/group w/o lift N/A  CCA N/A | | | | Size/group w/o lift 31  CCA 1500 | | | |
| 1400 CCA 12 volt minimum to be mounted in body battery compartment w/lift. | | | Size/group w/lift 31  CCA 1500 | | | Size/group w/lift  CCA | | | | Size/group w/lift 31  CCA 1500 | | | |
| Battery Compartment | Battery storage tray must be large enough to accommodate batteries as specified in chassis section. | | | | | | | Swing out | | | | Roll out | | |
| Brakes | Hydraulic disc. Refer to Washington State School Bus Specifications Manual. | | | | | | | Size Front 2.60 Rear 2.60 | | | | | | |
| Door, Service | Power operated. | | | | | | | Air  Electric  Other | | | | Folding  Split, Outward opening  Other | | |
| Engine | Diesel and Propane—180 H.P. minimum.  Gas—210 H.P. minimum. | | ***Diesel*** | | | ***Gas*** | | | | ***Propane*** | | | | |
| Engine mfr. DETROIT DD5 | | | Engine mfr. N/A | | | | Engine mfr. AGILITYI | | | | |
| Model or liters DD5 | | | Model or liters | | | | Model or liters 8.0L | | | | |
| Net torque 560 @ 1400 R.P.M | | | Net torque      @      R.P.M | | | | Net torque 495 @ 3100 R.P.M | | | | |
| Net H.P. 200 @ 2200 R.P.M | | | Net H.P.      @      R.P.M | | | | Net H.P. 339 @ 4100 R.P.M | | | | |
| Engine Heater | Engine manufacturer’s recommended in-block heater. | | | | | | | Watts 750 | | | | | | Volts 115 |
| Mfr. PHILLIPS | | | | | | |
| Engine Temperature | To be controlled electronically, by fan clutch/drive, or shutters. | | | | | | | Mfr. EATON | | | | | | Electronic |
| Fan clutch | | | | | | Shutters |
| Fuel Tank | Diesel and Gas—60 gallon minimum.  Propane—largest available. | | | | ***Diesel*** | | | ***Gas*** | | | | | ***Propane*** | |
| Capacity 60 USABLE | | | Capacity N/A | | | | | Capacity 67 USABLE | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification**  **TYPE C60—BID AS 48 PASSENGER,**  **DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift buses for 35–60 capacity.** | Vendor: SCHETKY NW SALES,INC. |
|  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | |  | |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | |
| Heaters | Minimum of 210,000 BTU total. Shutoff valves at engine for all heaters. Two-speed motors. Must include recirculating pump. | Left-front B.T.U. 84,000 | | Right-front B.T.U. 30,600 |
| Center B.T.U. 50,000 | | Rear B.T.U. 50,000 |
| Total B.T.U. 214,600 | |  |
| Hood | Tilt. | Fiberglass | | Metal |
| Lights | LED (Light Emitting Diode). Includes Clearance Lights, Stop Lights–7”, Tail Lights, Turn Signals, Eight-Light System, and Dome-Light System. | Check if as specified  If not, explain | | |
| P.A. System | AM/FM/PA radio with 2 interior and 1 exterior speakers. | Mfr. PANASONIC | | |
| Model No. D106900003 INCL CD PLAYER | | |
| Seat Spacing | To permit specified passenger capacity based on an average center-to-center seat spacing of at least 27.5”. | Inside measurement from rear of stepwell to  appropriate point at rear of passenger  seating area: w/o lift 247.1" w/lift 217.0" | | |
| Mfg.’s C/C seat measurement of vehicle  (inches): w/o lift 28.8 w/lift 28.8 | | |
| Steering Wheel | Tilt and telescoping column. | Check if as specified | | |
| Step Tread | Studded or pebbled top tread covering. | Mfr. RCA | | |
| Tires | 6 first quality, radial ply. No low profile tires. | Mfr. HANKOOK | | |
| Size 11R22.5 | | |
| Load range G | | |
| Toolbox | Exterior, manufacturer standard. | Size (cubic feet) 6.9 | | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification**  **TYPE C60—BID AS 48 PASSENGER,**  **DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift buses for 35–60 capacity.** | Vendor: SCHETKY NW SALES, INC. |
|  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | |  | | | | | | |  | |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | | | | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | | |
| Transmission | Diesel and Propane: Automatic—Allison, PTS 2500 or equal.  Gas: Automatic—manufacturer’s standard compatible with H.P. and torque rating of engine bid. | | | ***Diesel*** | ***Gas*** | | | | | ***Propane*** |
| Mfr. ALLISON | Mfr. N/A | | | | | Mfr. ALLISON |
| Model no. PTS 2500 | Model no. N/A | | | | | Model no. PTS 2300 |
| Net input 550 GROSS INPUT | Net input N/A | | | | | Net input 505 GROSS |
| Net input H.P. 300 | Net input H.P. N/A | | | | | Net input H.P. 325 |
| Two-way Communications | 45-watt, VHF, mil. spec. | | | | | Mfr. KENNWOOD | | | | |
| Model No. TK-7302HVK 50 WATT VHF | | | | |
| Wheels | 6 to be compatible with tire size. | | | | | Size 22.5 | | | | |
| Rim width 7.5 | | | | |
|  | | | **SPECIAL NEEDS REQUIREMENTS—CHASSIS AND BODY** | | | | |  | | |
| Wheelchair  Lift—Installed | Must meet state specification. Platform shall be a minimum of 32” x 52”. | | | | | Mfr. BRUAUN | | | | |
| Model No. NCL917IB-2 | | | | |
| Wheelchair/ Occupant Tie-down System—Installed | Must meet state specification. | | | | | Mfr. SURE-LOK | | | | |
| Model No. FF627S-4C-3 | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification**  **TYPE C60—BID AS 48 PASSENGER,**  **DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift buses for 35–60 capacity.** | Vendor: SCHETKY NW SALES, INC. |
|  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | |  |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | |
|  | **ADDITIONAL REQUIREMENTS—CHASSIS AND BODY** | |  |
| Line Setting Ticket | Legible copy of manufacturer’s Line Setting Ticket will be delivered with each vendor’s packet at the time of delivery of the bus. | Check if as specified | |
| Owner’s/Operator’s Handbook | One copy of the chassis manufacturer’s owner’s/operator’s handbook or manual will be furnished with each bus at time of delivery. | Check if as specified | |
| Repair Manuals | A complete set of chassis, engine, transmission, and body repair manuals, including wiring diagram for all components, will be made available at time of delivery, with instructions available on accessing repair materials. | Check if as specified | |
| Service and Cleaning | Cleaning and service by vendor prior to delivery will include:   * Chassis lubrication. * Check fluid levels: verify all are at recommended full levels. * Cooling system protected at -20°F. * Interior and exterior will be clean (including glass). * All systems (electric, air, hydraulic, mechanical and manual) be inspected to ensure proper operation at time of delivery. * All components and accessories will be installed and operational at time of delivery. | Check if as specified | |
| Warranty | A complete copy of all warranty agreements will be furnished at time of delivery. | Check if as specified | |

|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo  **2018-19** | STUDENT TRANSPORTATION  Old Capitol Building  PO BOX 47200  Olympia, WA 98504-7200  (360) 725-6120 TTY (360) 664-3631  **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION**  **TYPE C60—BID AS 48 PASSENGER (DIESEL)** | | |
|  | |  | |
| VENDOR’S COMPANY NAME  SCHETKY NW SALES, INC. | | REPRESENTATIVE’S NAME  KIM HEVIA | TELEPHONE NUMBER  503-382-3126 |
| ADDRESS  8430 KILLINGSWORTH ST.  PORTLAND, OR. 97220 | | Estimated delivery date to school district from time purchase order is received: 180-120 DAYS ARO  Firm where engine and chassis can be  serviced or repaired and parts obtained: SCHETKY NW SALES, INC.  Firm where body can be serviced or repaired and parts obtained: SCHETKY NW SALES, INC. | |
|  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **BODY** | | | | |
| MAKE  THOMAS BUILT BUSES | | Warranty: Years 3  Miles 50,000  Seat color: GRAY  Floor color: BLACK | Inside measurement from rear of stepwell to appropriate point at  rear of passenger seating area:  w/o lift 247.1" w/lift 217.1" | Equipped seating capacity:  w/o lift 48 w/lift 28  Overall vehicle length (inches):  w/o lift 358 w/lift 329.9 |
| MODEL  221TS W/O LIFT  191TS W / LIFT | YEAR  2020 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CHASSIS** | | | **ENGINE** | | |
| MAKE  FREIGHTLINER | | Warranty: Years 3  Miles 50,000 | MANUFACTURER  DETROIT | | Torque: 560 @ 1400 RPM  H.P.: 200 @ 2200 RPM |
| MODEL  B2106 | YEAR  2020 | Wheel base: 199" | MODEL  DD5 | YEAR  NEW | C.I.D. or Liters: 5.1L  Fuel type: DIESEL |
| **TRANSMISSION** | | | Warranty: Years 5  Miles 100,000  Number of cylinders: 4  Inline X V-type | | Battery type/grp: 31 31  Number batteries: 2 2  Total CCA: 1500 1500 |
| MANUFACTURER  ALLISON | | Speeds forward: 5 |
| MODEL  PTS 2500 | | Warranty: Years 7  Miles UNLTD |

|  |  |
| --- | --- |
| **QUOTED PRICE** | |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).  Diesel Bid—w/o lift $ 90,254.00 Diesel Bid—w/lift $ 93,556.00 | |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo  **2018-19** | STUDENT TRANSPORTATION  Old Capitol Building  PO BOX 47200  Olympia, WA 98504-7200  (360) 725-6120 TTY (360) 664-3631  **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION**  **TYPE C60—BID AS 48 PASSENGER (GAS)** | | |
|  | |  | |
| VENDOR’S COMPANY NAME  SCHETKY NW SALES, INC. | | REPRESENTATIVE’S NAME  KIM HEVIA | TELEPHONE NUMBER  503-382-3126 |
| ADDRESS  8430 NE KILLINGSWORTH ST.  PORTLAND, OR. 97220 | | Estimated delivery date to school district from time purchase order is received: 180-220 DAYS ARO  Firm where engine and chassis can be  serviced or repaired and parts obtained: SCHETKY NW SALES, INC.  Firm where body can be serviced or repaired and parts obtained: SCHETKY NW SALES, INC. | |
|  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **BODY** | | | | |
| MAKE  N/A | | Warranty: Years  Miles  Seat color:  Floor color: | Inside measurement from rear of stepwell to appropriate point at  rear of passenger seating area:  w/o lift       w/lift | Equipped seating capacity:  w/o lift       w/lift  Overall vehicle length (inches):  w/o lift       w/lift |
| MODEL  N/A | YEAR  N/A |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CHASSIS** | | | **ENGINE** | | |
| MAKE  N/A | | Warranty: Years  Miles | MANUFACTURER | | Torque:       @       RPM  H.P.:       @       RPM |
| MODEL  N/A | YEAR  N/A | Wheel base: | MODEL | YEAR | C.I.D. or Liters:  Fuel type: |
| **TRANSMISSION** | | | Warranty: Years  Miles  Number of cylinders:  Inline       V-type | | Battery type/grp:  Number batteries:  Total CCA: |
| MANUFACTURER | | Speeds forward: |
| MODEL | | Warranty: Years  Miles |

|  |  |
| --- | --- |
| **QUOTED PRICE** | |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).  Gas Bid—w/o lift $ NO BID Gas Bid—w/lift $ NO BID | |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo  **2018-19** | STUDENT TRANSPORTATION  Old Capitol Building  PO BOX 47200  Olympia, WA 98504-7200  (360) 725-6120 TTY (360) 664-3631  **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION**  **TYPE C60—BID AS 48 PASSENGER (PROPANE)** | | |
|  | |  | |
| VENDOR’S COMPANY NAME  SCHETKY NW SALES, INC. | | REPRESENTATIVE’S NAME  KIM HEVIA | TELEPHONE NUMBER  503-382-3126 |
| ADDRESS  8430 KILLINGSWORTH ST.  PORTLAND, OR. 97220 | | Estimated delivery date to school district from time purchase order is received: 180-220 DAYS ARO  Firm where engine and chassis can be  serviced or repaired and parts obtained: SCHETKY NW SALES, INC.  Firm where body can be serviced or repaired and parts obtained: SCHETKY NW SALES, INC. | |
|  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **BODY** | | | | |
| MAKE  THOMAS BUILT BUSES | | Warranty: Years 3  Miles 50,000  Seat color: GRAY  Floor color: BLACK | Inside measurement from rear of stepwell to appropriate point at  rear of passenger seating area:  w/o lift 247.1 " w/lift 217.1" | Equipped seating capacity:  w/o lift 48 w/lift 43  Overall vehicle length (inches):  w/o lift 358 w/lift 357 |
| MODEL  251TS W / O LIFT  251TS W/ LIFT | YEAR  2019/2020 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CHASSIS** | | | **ENGINE** | | |
| MAKE  FREIGHTLINER | | Warranty: Years 3  Miles 50,000 | MANUFACTURER  AGILITY | | Torque: 495 @ 3100 RPM  H.P.: 339 @ 4100 RPM |
| MODEL  B2106 | YEAR  2019/2020 | Wheel base: 199" W/O LIFT / 219" W/LIFT | MODEL  488 LPG | YEAR  NEW | C.I.D. or Liters: 488  Fuel type: PROPANE |
| **TRANSMISSION** | | | Warranty: Years 5  Miles 100,000  Number of cylinders: 8  Inline       V-type X | | Battery type/grp: 31 31  Number batteries: 2 2  Total CCA: 1500 1500 |
| MANUFACTURER  ALLISON | | Speeds forward: 5 |
| MODEL  PTS 2300 | | Warranty: Years 5  Miles UNLTD |

|  |  |
| --- | --- |
| **QUOTED PRICE** | |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).  Propane Bid—w/o lift $ 98,769.00 Propane Bid—w/lift $ 102,740.00 | |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

PART II

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification**  **DISTRICT-SUPPORTED OPTIONS**  **C60**  **C77**  **D60**  **D84**  **Use this document to bid both non-lift and lift buses.** | Vendor: SCHETKY NW SALES, INC. |
|  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | |  | |
| **ITEM** | Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the district cost. | | |
| Activity Securement Seating | 2-passenger position seats with lap-shoulder belts in all passenger positions. | Passenger Capacity 32 | | |
| Cost $ 825.00 PER SEAT | | |
| Air Conditioning | To cool passenger compartment as required in the Washington State School Bus Specifications manual. | Mfr. CARRIER AC-572MAX 70K BTU | | |
| Cost $ 5,640.00 | | |
| Alternate Fuel | Must comply with power and gradeability formula. Refer to Washington State School Bus Specifications manual. Must comply with all of the requirements of FMVSS No. 305. | Mfr. IMPCO | | |
| CNG | CNG Cost $ 36,000.00 | | |
| Electric | Electric Cost $ 375,000.00 | | |
| Alternator | Available options. | Cost $ 580.00 Capacity 270 4949PA PADMOUNT | | |
| Cost $ 650.00 Capacity 275 40 SI | | |
| Cost $ 780.00 Capacity 320 4962PA DMOUNT | | |
| Anti-spray Device | Rubber fender extenders. | Type C: Cost $ 185.00 | | |
| Type D: Cost $ | | |
| Back-up Alarm | Must meet state specification. | Mfr. THOMAS | | |
| Cost $ 155.00 | | |
| Brakes | 4-wheel hydraulic disk brake. | Cost $ INCLUDED | | Deduct $ N/A |
| Brakes | Air, Drum or Disc. Refer to Washington State School Bus Specifications manual. | Disc Cost $ 3,20.00 | | Disc Deduct $ N/A |
| Drum Cost $ 2,950.00 | | Drum Deduct $ N/A |
| Color | Exterior white roof. | Cost $ 558.00 | | |
| Door Locks | Vandal lock system on all exterior doors. | Cost $ 295.00 | | |
| Driver’s Seat | Suspension type, 6-way adjustable, with lumbar adjustment. Cloth panel covers. | ***Non-Air*** | | ***Air*** |
| Mfr. NATIONAL | | Mfr. NATIONAL |
| Cost $ INCLUDED | | Cost $ 495.00 |
| Fire Suppression System | Jomarr VT-6-E-NAF, or equal engine compartment fire suppression system of appropriate size to be installed according to manufacturer recommendation. | Mfr. JOMARR | | |
| Cost $ 3,800.00 | | |

PART II (cont.)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification**  **DISTRICT-SUPPORTED OPTIONS**  **C60  C77  D60  D84**  **Use this document to bid both non-lift and lift buses.** | Vendor: SCHETKY NWSALES, INC. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  | | |
| **ITEM** | Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the district cost. | |
| Floor Color | Nonstandard color. | | Cost $ 530.00 | |
| Fuel Tank | Larger fuel capacity (CNG only). | | Size: N/A | Cost $ |
| Fuel Tank | Larger fuel capacity (Diesel only). | | Size: 100 GALLEN | Cost $ 590.00 |
| Fuel Tank | Larger fuel capacity (Propane only). | | Size: N/A | Cost $ |
| Headlights | Halogen. | | Cost $ INCLUDED | |
| Headlights | L.E.D. | | Cost $ 622.00 FACTORY INSTALLED | |
| Heater (Auxiliary water) | Auxiliary fuel-fired heating systems. Refer to Washington State School Bus Specifications Manual, page 27. | | Brand: WEBASTO Model: 45K BTU | |
| Cost $ 3,760.00 | |
| Noise Reduction | Exceeding minimum specifications. | | Driver compartment Cost $ 150.00 | |
| Engine compartment Cost $ 190.00 | |
| Full acoustical headliner Cost $ 725.00 | |
| Retarder | Manufacturer’s standard. | | Driveline  Cost $ 150.00 | |
| Exhaust  Cost $ DIESEL ONLY | |
| Transmission  Cost $ | |
| Seat Belt Ready Seat | 3-passenger position seat with securement belts. | | Cost $ 695.00 PER SEAT | |
| Seating System | Identical, non-lift bus with lap-shoulder seat belt system installed in all positions. | | 2 by 2 Cost $ 6,900.00 | |
| Capacity 32 | |
| 3 by 2 Cost $ 7,125.00 | |
| Capacity 40 | |
| 3 by 3 Cost $ 7,700.00 | |
| Capacity 48 | |

PART II (cont.)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification**  **DISTRICT-SUPPORTED OPTIONS**  **C60  C77  D60  D84**  **Use this document to bid both non-lift and lift buses.** | Vendor: SCHETKY NW SALES, INC. |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  | | | |
| **ITEM** | Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the district cost. | | |
| Storage Compartments | Largest available for unit bid. | | Left-side 17.8 cubic feet. | | |
| Cost $ 1,450.00 | | |
| Right-side 17.8 cubic feet. | | |
| Cost $ 1,450.00 | | |
| Push-thru N/A cubic feet. | | |
| Cost $ | | |
| Strobe Light | Exterior roof mounted white strobe light. | | Mfr. THOMAS | | |
| Model No. DOUBLE FLASH | | |
| Cost $ 175.00 4.9" H | | |
| Student Protection System—Installed | Electronic system to insure driver post-trip inspection of passenger compartment. | | Mfr. THOMAS | | |
| Model No. D403000000 | | |
| Cost $ 245.00 | | |
| Suspension | Air ride (Air brake system only). | | ***Front*** | ***Rear*** | |
| Cost $ N/A | Cost $ 2,975.00 | |
| Toolbox | Interior, manufacturer standard. | | Cost $ 50.00 | Deduct $ N/A | |
| Traction Device | Automatic chains. | | Mfr. INSTA CHAINS | | |
| Cost $ 2,400.00 | | |
| Traction Device | Sanders. | | Capacity 158LBS | | |
| Cost $ 3,120.00 | | |
| Transmission | Automatic—Allison, PTS 3000 or equal. | | Mfr. ALLISON | | |
| Model No. 3000PTS | | |
| Cost $ 5,300.00 | | |
| Vehicle Securement System | Must meet state specification. | | Mfr. SAFTY- BRAKE | | Cost $ 1,050.00 |

PART II (cont.)

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **State Price Quote Specification**  **DISTRICT-SUPPORTED OPTIONS**  **C60  C77  D60  D84**  **Use this document to bid both non-lift and lift buses.** | Vendor: SCHETKY NW SALES, INC. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  | | |
| **ITEM** | Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the district cost. | |
| Video Camera Systems—Installed | Digital audio/video system for monitoring the passenger compartment with more than two cameras. | | Mfr. AMERICAN BUS VIDEO | |
| Model No. RSD4MX-4 | |
| Cost $ 2,200.00 How many cameras 4 | |
| Video Camera Systems—Stop Sign Camera—Installed | Must meet state specification. | | ***Stand Alone System*** | ***Added to Interior System*** |
| Mfr. AMERICAN BUS VIDEO | Mfr. AMERICAN BUS VIDEO |
| Model No. RSD4HD-1 | Model No. SACA 12MM |
| Cost $ 1,175.00 | Cost $ 240.00 |
| How many cameras 1 | How many cameras 1 |
| Warning Light Monitor | 16 light monitoring system. | | ***Incandescent*** | ***LED Lights*** |
| Cost $ 240.00 | Cost $ 240.00 |
| Additional Wheelchair/Occupant Tie-down System—Installed | Must meet state specification. | | Mfr. SURE-LOK | |
| Model No. FF627S-4C-3 | |
| Cost per station $ 792.00 WITH FLOOR POCKETS | |
| Windows | Laminated passenger-compartment side or rear glass. | | Side Cost $ 625.00 | |
| Rear Cost $ 325.00 | |
| Both Cost $ 950.00 | |
| Windows | Tinted. | | Cost $ 675.00 | |
| Windows | Thermal pane, left of driver and service door. | | Cost $ 770.00 | |