|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo  **2018-19** |  |  | **PART I** |
|  | **State Price Quote Specification**  **TYPE A— DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: BRYSON SALES & SERVICE OF WASHINGTON INC.  Mfr.: MICRO BIRD |
|  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  | | | |  | |
| **ITEM** | | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | |
| Seating Capacity | | Maximum passenger capacity based upon an average center-to-center seat spacing of at least 27.5” with a lap-shoulder belt for each seating position. | ***Gas*** | ***Diesel*** | | ***Propane*** |
| Capacity w/o lift 22 | Capacity w/o lift 22 | | Capacity w/o lift 28 |
| Capacity w/lift 13 | Capacity w/lift 13 | | Capacity w/lift 13 |
| Alternator | | 145 amp minimum. Lift-equipped or air-conditioned. Manufacturer recommended capacity. | | Mfr. DELCO / FORD / FORD | | |
| Amps output w/o lift or A.C. 220 / 210 /210 | | |
| Amps output w/lift or A.C. 220 / 210 / 210 | | |
| Auxiliary Automatic Transmission Cooler | | 10,000 lb. Hayden or equal. | ***Gas*** | ***Diesel*** | | ***Propane*** |
| Mfr. GM | Mfr. FORD | | Mfr. FORD |
| Lbs. rating 10,000 | Lbs. rating 10,000 | | Lbs. rating 10,000 |
| Axle—Front | | Manufacturer’s recommendation. | ***Gas*** | ***Diesel*** | | ***Propane*** |
| Mfr. GM | Mfr. FORD | | Mfr. FORD |
| Capacity 4300 | Lbs. rating 4130 | | Lbs. rating 5000 |
|  | |  | Indepen. suspens. | Indepen. suspens. | | Indepen. suspens. |
| Axle—Rear | | Manufacturer’s recommendation. | ***Gas*** | ***Diesel*** | | ***Propane*** |
| Mfr. GM | Mfr. FORD | | Mfr. FORD |
| Capacity 8600 | Capacity 6230 | | Capacity 9600 |
| Axle Ratio | | Must comply with power and gradeability formula. Refer to Washington State School Bus Specifications Manual. | ***Gas*** | ***Diesel*** | | ***Propane*** |
| Ratio 3.73 | Ratio 3.73 | | Ratio 4.56 |
| Back-up Lights | | All required backup lights to be LED (Light Emitting Diode). Refer to Washington State School Bus Specification’s Manual. | | Round:  Diameter 4"  Other:  Square inches | | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification**  **TYPE A— DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: BRYSON SALES & SERVICE OF WASHINGTON INC.  Mfr.: MICRO BIRD |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | | | |  | | | |
| **ITEM** | | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | | | |
| Battery(ies) | | 535 CCA 12 volt minimum for gas and propane w/o lift.  1070 CCA 12 volt minimum for diesel or any bus w/lift. | | ***Gas/Propane w/o lift*** | | | | ***Diesel or any bus w/lift*** |
| CCA GAS 1200 / PROPANE 650 | | | | CCA DIESEL 1520 |
| Brakes | | Hydraulic: Drum or Disc. Refer to Washington State School Bus Specifications Manual. | ***Gas*** | ***Diesel*** | | | ***Propane*** | |
| Front Disc | Front Disc | | | Front Disc | |
| Drum | Drum | | | Drum | |
| Rear Disc | Rear Disc | | | Rear Disc | |
| Drum | Drum | | | Drum | |
| Drum Size | Drum Size | | | Drum Size | |
| Doors, Service | | Power operated. | | Air  Folding  Electric  Split, Outward Opening  Other | | | | |
| Engine | | Gas and Propane—3.7 liters minimum.  Diesel—130 H.P. minimum. | ***Gas*** | ***Diesel*** | | ***Propane*** | | |
| Engine mfr. GM | Engine mfr. FORD | | Engine mfr. FORD | | |
| Liters 6.0L | H.P. 185 | | Liters 6.8L | | |
| Engine Heater | | Diesel only—engine manufacturer’s recommended in-block heater. | | Watts 400 | | | | Volts 12 |
| Mfr. FORD | | | | |
| Fuel Tank | | Gas and Diesel—25 gallon minimum.  Propane—largest available. | | ***Gas/Diesel*** | | | | ***Propane*** |
| Capacity GAS 33 / DIESEL 40 | | | | Capacity 40 |
| Hand Throttle | | Diesel only—locking type, electronic, or immediate acting electric fast idle. | | Vernier | | | | Electric |
| T type | | | | Electronic |
| Heaters | | Front—manufacturer’s standard. Rear—40,000 B.T.U. minimum. | | Rear B.T.U. w/o lift 42,000  Rear B.T.U. w/lift 42,000 | | | | |
| Lights | | LED (Light Emitting Diode). Includes Clearance Lights, Stop Lights–7”, Tail Lights, Turn Signals, Eight-Light System, and Dome-Light System. | | Check if as specified  If not, explain | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification**  **TYPE A— DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: BRYSON SALES & SERVICE OF WASHINGTON INC.  Mfr.: MICRO BIRD |
|  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | | |  | |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | |
| P.A. System | AM/FM/PA radio with 2 interior and 1 exterior speakers. | | Mfr. MITO | | |
| Model No. 07-SPF-210408 | | |
| Seat Spacing | To permit specified passenger capacity based on an average center-to-center seat spacing of at least 27.5”. | | Inside measurement from rear of stepwell to  appropriate point at rear of passenger seating  area: w/o lift 135 w/lift 135 | | |
| Mfg.’s C/C seat measurement of  vehicle (inches): w/o lift 27.5" w/lift 30" | | |
| Steering Wheel | Tilt. | | Check if as specified | | |
| Step Tread | Studded or pebbled top tread covering. | | Mfr. SMI | | |
| Tires | 6 first quality, radial ply. | | Mfr. ONE OF FIVE MAJOR BRANDS | | |
| Size LT 225 75R 16E BSW | | |
| Load range D | | |
| Toolbox | Exterior, manufacturer standard. | | Size (cubic feet) 1.20 | | |
| Transmission | Automatic—manufacturer’s standard compatible with H.P. and torque rating of engine bid. | ***Gas*** | ***Diesel*** | | ***Propane*** |
| Mfr. GM | Mfr. FORD | | Mfr. FORD |
| Model no. 6L90 | Model no. 6R80 | | Model no. 6R80 |
| Two-way Communications | 45-watt, VHF, mil. spec. | | Mfr. KENWOOD | | |
| Model No. TK7302 | | |
| Wheels | 6 to be compatible with tire size. | | Size 16" | | |
| Rim width 6" | | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification**  **TYPE A— DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: BRYSON SALES & SERVICE OF WASHINGTON INC.  Mfr.: MICRO BIRD |
|  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | |  | |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | |
|  | **SPECIAL NEEDS REQUIREMENTS—CHASSIS AND BODY** | |  | |
| Wheelchair  Lift—Installed | Must meet state specification. Platform shall be a minimum of 32” x 52”. | Mfr. BRAUN | | |
| Model No. NCL917FIB3454HB-2 | | |
| Wheelchair/Occupant Tie-down System—Installed | Must meet state specification. | Mfr. Q-STRAINT | | |
| Model No. Q-8100-A1 SLIDE & CLICK | | |
|  | **ADDITIONAL REQUIREMENTS—CHASSIS AND BODY** | | |  |
| Line Setting Ticket | Legible copy of manufacturer’s Line Setting Ticket will be delivered with each vendor’s packet at the time of delivery. | Check if as specified | | |
| Owner’s/Operator’s Handbook | One copy of the chassis manufacturer’s owner’s/operator’s handbook or manual will be furnished with each bus at delivery. | Check if as specified | | |
| Repair Manuals | A complete set of chassis, engine, transmission, and body repair manuals, including wiring diagram for all components, will be made available at time of delivery, with instructions available on accessing repair materials. | Check if as specified | | |
| Service and Cleaning | Cleaning and service by vendor prior to delivery will include:   * Chassis lubrication. * Check fluid levels: verify all are at recommended full levels. * Cooling system protected at -20°F. * Interior and exterior will be clean (including glass). * All systems (electric, air, hydraulic, mechanical and manual) be inspected to ensure proper operation at time of delivery. * All components and accessories will be installed and operational at time of delivery. | Check if as specified | | |
| Warranty | A complete copy of all warranty agreements will be furnished at time of delivery. | Check if as specified | | |

|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo  **2018-19** | STUDENT TRANSPORTATION  Old Capitol Building  PO BOX 47200  Olympia, WA 98504-7200  (360) 725-6120 TTY (360) 664-3631  **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION**  **TYPE A—DIESEL** | | |
|  | |  | |
| VENDOR’S COMPANY NAME  BRYSON SALES & SERVICE OF WASHINGTON INC. | | REPRESENTATIVE’S NAME  ROBERT KANTER | TELEPHONE NUMBER  425-953-2820 |
| ADDRESS  2407 GIBSON RD  EVERETT, WA 98204 | | Estimated delivery date to school district from time purchase order is received: 150 - 180 DAYS ARO  Firm where engine and chassis can be  serviced or repaired and parts obtained: BRYSON SALES & SERVICE OF WASHINGTON INC.  Firm where body can be serviced or repaired and parts obtained: BRYSON SALES & SERVICE OF WASHINGTON INC. | |
|  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **BODY** | | | | |
| MAKE  MICRO BIRD | | Warranty: Years 3  Miles 36,000  Seat color: BROWN  Floor color: GRAY | Inside measurement from rear of stepwell to appropriate point at  rear of passenger seating area:  w/o lift 156" w/lift 156" | Equipped seating capacity:  w/o lift 22 w/lift 13  Overall vehicle length (inches):  w/o lift 253" w/lift 253" |
| MODEL  MB II | YEAR  2019 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CHASSIS** | | | **ENGINE** | | |
| MAKE  FORD | | Warranty: Years 5  Miles 60,000 | MANUFACTURER  FORD | | Torque: 350 @ 1500 RPM  H.P.: 185 @ 3000 RPM |
| MODEL  10,360 | YEAR  2019 | Wheel base: 156" | MODEL  3.2L | YEAR  2019 | Fuel type: DIESEL |
| **TRANSMISSION** | | | Warranty: Years 5  Miles 60,000  Number of cylinders: 6  Inline       V-type X | | Battery type/grp: 70 AMP  Number batteries: 1  Total CCA: 760 |
| MANUFACTURER  FORD | | Speeds forward: 6 |
| MODEL  6R80 | | Warranty: Years 5  Miles 60,000 |

|  |  |
| --- | --- |
| **QUOTED PRICE** | |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).  Diesel Bid—w/o lift $ 64,211.00 Diesel Bid—w/lift $ 69,265.00 | |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo  **2018-19** | STUDENT TRANSPORTATION  Old Capitol Building  PO BOX 47200  Olympia, WA 98504-7200  (360) 725-6120 TTY (360) 664-3631  **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION**  **TYPE A—GAS** | | |
|  | |  | |
| VENDOR’S COMPANY NAME  BRYSON SALES & SERVICE OF WASHINGTON INC. | | REPRESENTATIVE’S NAME  ROBERT KANTER | TELEPHONE NUMBER  425-953-2820 |
| ADDRESS  2407 GIBSON RD  EVERETT, WA 98204 | | Estimated delivery date to school district from time purchase order is received: 150 - 180 DAYS ARO  Firm where engine and chassis can be  serviced or repaired and parts obtained: BRYSON SALES & SERVICE OF WASHINGTON INC.  Firm where body can be serviced or repaired and parts obtained: BRYSON SALES & SERVICE OF WASHINGTON INC. | |
|  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **BODY** | | | | |
| MAKE  MICRO BIRD | | Warranty: Years 3  Miles 36,000  Seat color: BROWN  Floor color: GRAY | Inside measurement from rear of stepwell to appropriate point at  rear of passenger seating area:  w/o lift 153.75" w/lift 153.75" | Equipped seating capacity:  w/o lift 22 w/lift 13  Overall vehicle length (inches):  w/o lift 262" w/lift 262" |
| MODEL  G5 | YEAR  2019 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CHASSIS** | | | **ENGINE** | | |
| MAKE  GM | | Warranty: Years 3  Miles 36,000 | MANUFACTURER  GM | | Torque: 360 @ 4000 RPM  H.P.: 300 @ 4400 RPM |
| MODEL  12300 / CG33803 | YEAR  2019 | Wheel base: 139" | MODEL  6.0L VORTEC | YEAR  2019 | Liters: 6.0L  Fuel type: GASOLINE |
| **TRANSMISSION** | | | Warranty: Years 3  Miles 36,000  Number of cylinders: 6  Inline       V-type X | | Battery type/grp: MAINT FREE  Number batteries: 1  Total CCA: 600 |
| MANUFACTURER  GM | | Speeds forward: 6 |
| MODEL  6L90 | | Warranty: Years 3  Miles 36,000 |

|  |  |
| --- | --- |
| **QUOTED PRICE** | |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).  Gas Bid—w/o lift $ 59,997.00 Gas Bid—w/lift $ 64,397.00 | |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo  **2018-19** | STUDENT TRANSPORTATION  Old Capitol Building  PO BOX 47200  Olympia, WA 98504-7200  (360) 725-6120 TTY (360) 664-3631  **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION**  **TYPE A—PROPANE** | | |
|  | |  | |
| VENDOR’S COMPANY NAME  BRYSON SALES & SERVICE OF WASHINGTON INC. | | REPRESENTATIVE’S NAME  ROBERT KANTER | TELEPHONE NUMBER  425-953-2820 |
| ADDRESS  2407 GIBSON RD  EVERETT, WA 98204 | | Estimated delivery date to school district from time purchase order is received: 150 - 180 DAYS ARO  Firm where engine and chassis can be  serviced or repaired and parts obtained: BRYSON SALES & SERVICE OF WASHINGTON INC.  Firm where body can be serviced or repaired and parts obtained: BRYSON SALES & SERVICE OF WASHINGTON INC. | |
|  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **BODY** | | | | |
| MAKE  MICRO BIRD | | Warranty: Years 3  Miles 36,000  Seat color: BROWN  Floor color: GRAY | Inside measurement from rear of stepwell to appropriate point at  rear of passenger seating area:  w/o lift 156" w/lift 156" | Equipped seating capacity:  w/o lift 22 w/lift 13  Overall vehicle length (inches):  w/o lift 253" w/lift 253" |
| MODEL  G5 | YEAR  2019 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CHASSIS** | | | **ENGINE** | | |
| MAKE  FORD | | Warranty: Years 5  Miles 60,000 | MANUFACTURER  FORD | | Torque: 457 @ 3250 RPM  H.P.: 362 @ 4750 RPM |
| MODEL  E450/14500 | YEAR  2019 | Wheel base: 158" | MODEL  6.8L | YEAR  2019 | Liters: 6.8L  Fuel type: PROPANE |
| **TRANSMISSION** | | | Warranty: Years 5  Miles 60,000  Number of cylinders: 10  Inline       V-type X | | Battery type/grp: 12V  Number batteries: 1  Total CCA: 750 |
| MANUFACTURER  FORD | | Speeds forward: 6 |
| MODEL  6R80 | | Warranty: Years 5  Miles 60,000 |

|  |  |
| --- | --- |
| **QUOTED PRICE** | |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).  Propane Bid—w/o lift $ 79,943.00 Propane Bid—w/lift $ 84,676.00 | |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART II** |
|  | **State Price Quote Specification**  **DISTRICT-SUPPORTED OPTIONS**  **TYPE A**  **Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: BRYSON SALES & SERVICE OF WASHINGTON, INC.  Mfr.: MICRO BIRD |
|  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | **CHASSIS** | | |  | | | |
| **ITEM** | Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the district cost. | | | |
| Small A | Type A bus—10,000 lbs or under GVWR chassis. | ***Gas*** | | | ***Diesel*** | | ***Propane*** |
| Deduct $744.07 | | | Deduct N/A | | Deduct N/A |
| Mfr. FORD T-SERIES | | | Mfr. N/A | | Mfr. N/A |
| Capacity w/o lift 16 | | | Capacity w/o lift N/A | | Capacity w/o lift N/A |
| Dual Wheel | | | Dual Wheel | | Dual Wheel |
| Single Wheel | | | Single Wheel | | Single Wheel |
| Air Conditioning | To cool passenger compartment as required in the Washington State School Bus Specifications manual. | | | Mfr. MCC | | | |
| Cost $ 2405.00 | | | |
| Alternate Fuel | Must comply with power and gradeability formula. Refer to Washington State School Bus Specifications manual. Must comply with all of the requirements of FMVSS No. 305. | | | Mfr. MICRO BIRD | | | |
| CNG | CNG Cost $ N/A | | | |
| Electric | Electric Cost $ 150000.00 | | | |
| Back-up Alarm | Must meet state specification. | | | Mfr. ECCO | | | |
| Cost $ 137.00 | | | |
| Color | Exterior white roof. | | | Cost $ INCLUDED | | | |
| Steering Wheel | Tilt and telescoping column. | | | Cost $ INCLUDED | | | |
| Strobe Light | Exterior roof mounted white strobe light. | | | Mfr. ECCO | | | |
| Model No. 7460 LED CLEAR LENS | | | |
| Cost $ 286.00 | | | |
| Student Protection System—Installed | Electronic system to insure driver post-trip inspection of passenger compartment. | | Mfr. DORAN | | | | |
| Model No. SLEEPING CHILD CHECK | | | | |
| Cost $ 244.00 | | | | |
| Toolbox | Interior, manufacturer standard. | | Cost $ INCLUDED | | | Deduct $ 56.00 | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART II (cont.)** |
|  | **State Price Quote Specification**  **DISTRICT-SUPPORTED OPTIONS**  **TYPE A**  **Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: BRYSON SALES & SERVICE OF WASHINGTON, INC.  Mfr.: MICRO BIRD |
|  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  | | |
| **ITEM** | Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the district cost. | |
| Video Camera Systems—Installed | Digital audio/video system for monitoring the passenger compartment with more than two cameras. | | Mfr. SEON | |
| Model No. TH-4 | |
| Cost $ 1958.00 How many cameras 3 | |
| Video Camera Systems—Stop Sign Camera—Installed | Must meet state specification. | | ***Stand Alone System*** | ***Added to Interior System*** |
| Mfr. SEON | Mfr. SEON |
| Model No. TH-4 | Model No. TH-4 |
| Cost $ 1440.00 | Cost $ 354.00 |
| How many cameras 1 | How many cameras 1 |
| Warning Light Monitor | 16 light monitoring system. | | ***Incandescent*** | ***LED Lights*** |
| Cost $ 440.00 | Cost $ 440.00 |
| Additional Wheelchair/Occupant Tie-down System—Installed | Must meet state specification. | | Mfr. Q-STRAINT | |
| Model No. Q-8100-A1 | |
| Cost per station $ 869.00 | |
| Windows | Laminated passenger-compartment side or rear glass. | | Side Cost $ 900.00 | |
| Rear Cost $ 654.00 | |
| Both Cost $ 1554.00 | |
| Windows | Tinted. | | Cost $ INCLUDED | |