|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo  **2019-2020** |  |  | **PART I** |
|  | **State Price Quote Specification**  **TYPE A— DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: Northwest Bus Sales  Mfr.: Starcraft |
|  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  | | | |  | |
| **ITEM** | | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | |
| Seating Capacity | | Maximum passenger capacity based upon an average center-to-center seat spacing of at least 27.5” with a lap-shoulder belt for each seating position. | ***Gas*** | ***Diesel*** | | ***Propane*** |
| Capacity w/o lift 26 | Capacity w/o lift 21 | | Capacity w/o lift |
| Capacity w/lift 18+1 wc | Capacity w/lift 12+1wc | | Capacity w/lift |
| Alternator | | 145 amp minimum. Lift-equipped or air-conditioned. Manufacturer recommended capacity. | | Mfr. GM / Diesel Ford | | |
| Amps output w/o lift or A.C. Gas 220/ Diesel 210 | | |
| Amps output w/lift or A.C. Gas 220 / Diesel 210 | | |
| Auxiliary Automatic Transmission Cooler | | 10,000 lb. Hayden or equal. | ***Gas*** | ***Diesel*** | | ***Propane*** |
| Mfr. GM | Mfr. Ford | | Mfr. |
| Lbs. rating 10,000 | Lbs. rating 10000 | | Lbs. rating |
| Axle—Front | | Manufacturer’s recommendation. | ***Gas*** | ***Diesel*** | | ***Propane*** |
| Mfr. GM | Mfr. Ford | | Mfr. |
| Capacity 4300 | Lbs. rating 4130 | | Lbs. rating |
|  | |  | Indepen. suspens. ☒ | Indepen. suspens. ☒ | | Indepen. suspens. ☐ |
| Axle—Rear | | Manufacturer’s recommendation. | ***Gas*** | ***Diesel*** | | ***Propane*** |
| Mfr. GM | Mfr. Ford | | Mfr. |
| Capacity 8000 | Capacity 7275 | | Capacity |
| Axle Ratio | | Must comply with power and gradeability formula. Refer to Washington State School Bus Specifications Manual. | ***Gas*** | ***Diesel*** | | ***Propane*** |
| Ratio 3.73 | Ratio 4.10 | | Ratio |
| Back-up Lights | | All required backup lights to be LED (Light Emitting Diode). Refer to Washington State School Bus Specification’s Manual. | | Round: ☒ Diameter 4.6"  Other: ☐ Square inches | | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification**  **TYPE A— DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: Northwest Bus Sales  Mfr.: Starcraft |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | | | |  | | | |
| **ITEM** | | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | | | |
| Battery(ies) | | 535 CCA 12 volt minimum for gas and propane w/o lift.  1070 CCA 12 volt minimum for diesel or any bus w/lift. | | ***Gas/Propane w/o lift*** | | | | ***Diesel or any bus w/lift*** |
| CCA 700 | | | | CCA 1520 |
| Brakes | | Hydraulic: Drum or Disc. Refer to Washington State School Bus Specifications Manual. | ***Gas*** | ***Diesel*** | | | ***Propane*** | |
| Front Disc ☒ | Front Disc ☒ | | | Front Disc ☐ | |
| Drum ☐ | Drum ☐ | | | Drum ☐ | |
| Rear Disc ☒ | Rear Disc ☒ | | | Rear Disc ☐ | |
| Drum ☐ | Drum ☐ | | | Drum ☐ | |
| Drum Size | Drum Size | | | Drum Size | |
| Doors, Service | | Power operated. | | ☐ Air ☐ Folding ☒ Electric  ☐ Split, Outward Opening ☐ Other | | | | |
| Engine | | Gas and Propane—3.5 liters minimum.  Diesel—130 H.P. minimum. | ***Gas*** | ***Diesel*** | | ***Propane*** | | |
| Engine mfr. GM | Engine mfr. Ford | | Engine mfr. | | |
| Liters 6.0 | H.P. 168 | | Liters | | |
| Engine Heater | | Diesel only—engine manufacturer’s recommended in-block heater. | | Watts 400 | | | | Volts 110 |
| Mfr. Ford | | | | |
| Fuel Tank | | Gas and Diesel—25 gallon minimum.  Propane—largest available. | | ***Gas/Diesel*** | | | | ***Propane*** |
| Capacity 25 | | | | Capacity |
| Hand Throttle | | Diesel only—locking type, electronic, or immediate acting electric fast idle. | | ☐ Vernier | | | | ☐ Electric |
| ☐ T type | | | | ☒ Electronic |
| Heaters | | Front—manufacturer’s standard. Rear—40,000 B.T.U. minimum. | | Rear B.T.U. w/o lift 65,000  Rear B.T.U. w/lift 65,000 | | | | |
| Lights | | LED (Light Emitting Diode). Includes Clearance Lights, Stop Lights–7”, Tail Lights, Turn Signals, Eight-Light System, and Dome-Light System. | | Check if as specified ☒  If not, explain | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification**  **TYPE A— DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: Northwest Bus Sales  Mfr.: Starcraft |
|  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | | |  | |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | |
| P.A. System | AM/FM/PA radio with 2 interior and 1 exterior speakers. | | Mfr. Jensen | | |
| Model No. BR550 / PA500 | | |
| Seat Spacing | To permit specified passenger capacity based on an average center-to-center seat spacing of at least 27.5”. | | Inside measurement from rear of stepwell to  appropriate point at rear of passenger seating  area: w/o lift Gas 160.1875 Diesel 170.375 w/lift Gas 160.1875 Diesel 170.375 | | |
| Mfg.’s C/C seat measurement of  vehicle (inches): w/o lift 28 w/lift 28 | | |
| Steering Wheel | Tilt. | | Check if as specified ☒ | | |
| Step Tread | Studded or pebbled top tread covering. | | Mfr. Koloseal | | |
| Tires | 6 first quality, radial ply. | | Mfr. OEM | | |
| Size Gas LT225-75R16E Diesel 195/75R16 | | |
| Load range E | | |
| Toolbox | Exterior, manufacturer standard. | | Size (cubic feet) 3.35 | | |
| Transmission | Automatic—manufacturer’s standard compatible with H.P. and torque rating of engine bid. | ***Gas*** | ***Diesel*** | | ***Propane*** |
| Mfr. GM | Mfr. Ford | | Mfr. |
| Model no. 6L90 | Model no. SelectShift | | Model no. |
| Two-way Communications | 45-watt, VHF, mil. spec. | | Mfr. Motorola | | |
| Model No. CM200D | | |
| Wheels | 6 to be compatible with tire size. | | Size 16 | | |
| Rim width Gas 6.5 Diesel 6 | | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART I (cont.)** |
|  | **State Price Quote Specification**  **TYPE A— DIESEL, GAS & PROPANE**  **Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: Northwest Bus Sales  Mfr.: Starcraft |
|  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | |  | |
| **ITEM** | **STATE-SUPPORTED SPECIFICATIONS**  Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the state cost. | | |
|  | **SPECIAL NEEDS REQUIREMENTS—CHASSIS AND BODY** | |  | |
| Wheelchair  Lift—Installed | Must meet state specification. Platform shall be a minimum of 32” x 52”. | Mfr. Braun | | |
| Model No. Century NCL919IB-2 | | |
| Wheelchair/Occupant Tie-down System—Installed | Must meet state specification. | Mfr. Qstraint | | |
| Model No. Q8101 - Q8-6326-A1 | | |
|  | **ADDITIONAL REQUIREMENTS—CHASSIS AND BODY** | | |  |
| Line Setting Ticket | Legible copy of manufacturer’s Line Setting Ticket will be delivered with each vendor’s packet at the time of delivery. | Check if as specified ☒ | | |
| Owner’s/Operator’s Handbook | One copy of the chassis manufacturer’s owner’s/operator’s handbook or manual will be furnished with each bus at delivery. | Check if as specified ☒ | | |
| Repair Manuals | A complete set of chassis, engine, transmission, and body repair manuals, including wiring diagram for all components, will be made available at time of delivery, with instructions available on accessing repair materials. | Check if as specified ☒ | | |
| Service and Cleaning | Cleaning and service by vendor prior to delivery will include:   * Chassis lubrication. * Check fluid levels: verify all are at recommended full levels. * Cooling system protected at -20°F. * Interior and exterior will be clean (including glass). * All systems (electric, air, hydraulic, mechanical and manual) be inspected to ensure proper operation at time of delivery. * All components and accessories will be installed and operational at time of delivery. | Check if as specified ☒ | | |
| Warranty | A complete copy of all warranty agreements will be furnished at time of delivery. | Check if as specified ☒ | | |

|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo  **2019-2020** | STUDENT TRANSPORTATION  Old Capitol Building  PO BOX 47200  Olympia, WA 98504-7200  (360) 725-6120 TTY (360) 664-3631  **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION**  **TYPE A—DIESEL** | | |
|  | |  | |
| VENDOR’S COMPANY NAME  Northwest Bus Sales | | REPRESENTATIVE’S NAME  Rob Goolsby | TELEPHONE NUMBER  800-231-7099 |
| ADDRESS  33207 Pacific Hwy S.  Federal Way, WA 98003 | | Estimated delivery date to school district from time purchase order is received: 150-180 Days  Firm where engine and chassis can be  serviced or repaired and parts obtained: Any Ford Dealer  Firm where body can be serviced or repaired and parts obtained: Northwest Bus Sales | |
|  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **BODY** | | | | |
| MAKE  Starcraft | | Warranty: Years 3  Miles 36000  Seat color: Grey  Floor color: Black | Inside measurement from rear of stepwell to appropriate point at  rear of passenger seating area:  w/o lift 170.375 w/lift 170.375 | Equipped seating capacity:  w/o lift 21 w/lift 12+1wc  Overall vehicle length (inches):  w/o lift 275.0625 w/lift 275.0625 |
| MODEL  Quest | YEAR  2020 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CHASSIS** | | | **ENGINE** | | |
| MAKE  Ford | | Warranty: Years 3  Miles 36000 | MANUFACTURER  Ford | | Torque: 299 @ 2000 RPM  H.P.: 168 @ 2550 RPM |
| MODEL  Transit Cutaway | YEAR  2020 | Wheel base: 156 | MODEL  2.0L | YEAR  2020 | Fuel type: Diesel |
| **TRANSMISSION** | | | Warranty: Years 5  Miles 60000  Number of cylinders: 4  Inline x V-type | | Battery type/grp: 12v 12v  Number batteries: 2 2  Total CCA: 1520 1520 |
| MANUFACTURER  Ford | | Speeds forward: 6 |
| MODEL  SelectShift | | Warranty: Years 5  Miles 60000 |

|  |  |
| --- | --- |
| **QUOTED PRICE** | |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).  Diesel Bid—w/o lift $ 63,317 Diesel Bid—w/lift $ 66,392 | |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo  **2019-2020** | STUDENT TRANSPORTATION  Old Capitol Building  PO BOX 47200  Olympia, WA 98504-7200  (360) 725-6120 TTY (360) 664-3631  **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION**  **TYPE A—GAS** | | |
|  | |  | |
| VENDOR’S COMPANY NAME  Northwest Bus Sales | | REPRESENTATIVE’S NAME  Rob Goolsby | TELEPHONE NUMBER  206-445-8591 |
| ADDRESS  33207 Pacific Hwy S  Federal Way, WA 98003 | | Estimated delivery date to school district from time purchase order is received: 150-180 Days  Firm where engine and chassis can be  serviced or repaired and parts obtained: Any GM Dealer  Firm where body can be serviced or repaired and parts obtained: Northwest Bus Sales | |
|  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **BODY** | | | | |
| MAKE  Starcraft | | Warranty: Years 3  Miles 36000  Seat color: Grey  Floor color: Black | Inside measurement from rear of stepwell to appropriate point at  rear of passenger seating area:  w/o lift 160.1875 w/lift 160.1875 | Equipped seating capacity:  w/o lift 26 w/lift 18+1wc  Overall vehicle length (inches):  w/o lift 266.3125 w/lift 266.3125 |
| MODEL  Quest | YEAR  2020 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CHASSIS** | | | **ENGINE** | | |
| MAKE  Chevrolet | | Warranty: Years 3  Miles 36000 | MANUFACTURER  GM | | Torque: 373 @ 4400 RPM  H.P.: 342 @ 5400 RPM |
| MODEL  Express Cutaway | YEAR  2020 | Wheel base: 139 | MODEL  Vortec | YEAR  2020 | Liters: 6.0  Fuel type: Gas |
| **TRANSMISSION** | | | Warranty: Years 5  Miles 100000  Number of cylinders: 8  Inline       V-type x | | Battery type/grp: 12v 12v  Number batteries: 2 2  Total CCA: 1430 1430 |
| MANUFACTURER  Chevrolet | | Speeds forward: 6 |
| MODEL  6L90 | | Warranty: Years 5  Miles 60000 |

|  |  |
| --- | --- |
| **QUOTED PRICE** | |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).  Gas Bid—w/o lift $ 58,522 Gas Bid—w/lift $ 60,782 | |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |  |  |
| --- | --- | --- | --- |
| OSPI Logo  **2019-2020** | STUDENT TRANSPORTATION  Old Capitol Building  PO BOX 47200  Olympia, WA 98504-7200  (360) 725-6120 TTY (360) 664-3631  **VEHICLE DATA SHEET AND OFFICIAL PRICE QUOTATION**  **TYPE A—PROPANE** | | |
|  | |  | |
| VENDOR’S COMPANY NAME | | REPRESENTATIVE’S NAME | TELEPHONE NUMBER |
| ADDRESS | | Estimated delivery date to school district from time purchase order is received:  Firm where engine and chassis can be  serviced or repaired and parts obtained:  Firm where body can be serviced or repaired and parts obtained: | |
|  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **BODY** | | | | |
| MAKE | | Warranty: Years  Miles  Seat color:  Floor color: | Inside measurement from rear of stepwell to appropriate point at  rear of passenger seating area:  w/o lift       w/lift | Equipped seating capacity:  w/o lift       w/lift  Overall vehicle length (inches):  w/o lift       w/lift |
| MODEL | YEAR |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CHASSIS** | | | **ENGINE** | | |
| MAKE | | Warranty: Years  Miles | MANUFACTURER | | Torque:       @       RPM  H.P.:       @       RPM |
| MODEL | YEAR | Wheel base: | MODEL | YEAR | Liters:  Fuel type: |
| **TRANSMISSION** | | | Warranty: Years  Miles  Number of cylinders:  Inline       V-type | | Battery type/grp:  Number batteries:  Total CCA: |
| MANUFACTURER | | Speeds forward: |
| MODEL | | Warranty: Years  Miles |

|  |  |
| --- | --- |
| **QUOTED PRICE** | |
| Quoted price is based upon payment within 30 days after delivery to the school district (without sales tax).  Propane Bid—w/o lift $ n/a Propane Bid—w/lift $ n/a | |
| VENDOR REPRESENTATIVE’S SIGNATURE | DATE |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART II** |
|  | **State Price Quote Specification**  **DISTRICT-SUPPORTED OPTIONS**  **TYPE A**  **Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: Northwest Bus Sales  Mfr.: Starcraft |
|  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | **CHASSIS** | | |  | | | |
| **ITEM** | Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the district cost. | | | |
| Small A | Type A bus—10,000 lbs or under GVWR chassis. | ***Gas*** | | | ***Diesel*** | | ***Propane*** |
| Deduct N/A | | | Deduct N/A | | Deduct N/A |
| Mfr. | | | Mfr. | | Mfr. |
| Capacity w/o lift | | | Capacity w/o lift | | Capacity w/o lift |
| Dual Wheel ☐ | | | Dual Wheel ☐ | | Dual Wheel ☐ |
| Single Wheel ☐ | | | Single Wheel ☐ | | Single Wheel ☐ |
| Air Conditioning | To cool passenger compartment as required in the Washington State School Bus Specifications manual. | | | Mfr. TransAir | | | |
| Cost $ 1850 | | | |
| Alternate Fuel | Must comply with power and gradeability formula. Refer to Washington State School Bus Specifications manual. Must comply with all of the requirements of FMVSS No. 305. | | | Mfr. n/a | | | |
| ☐ CNG | ☐ CNG Cost $ | | | |
| ☐ Electric | ☐ Electric Cost $ | | | |
| Back-up Alarm | Must meet state specification. | | | Mfr. Ecco 107 | | | |
| Cost $ 35.00 | | | |
| Color | Exterior white roof. | | | Cost $ STD | | | |
| Steering Wheel | Tilt and telescoping column. | | | Cost $ Tilt is STD | | | |
| Strobe Light | Exterior roof mounted white strobe light. | | | Mfr. Sound Off Signal | | | |
| Model No. 3107LCC | | | |
| Cost $ 207 | | | |
| Student Protection System—Installed | Electronic system to insure driver post-trip inspection of passenger compartment. | | Mfr. Child Checkmate | | | | |
| Model No. DLRH-1 | | | | |
| Cost $ 245 | | | | |
| Toolbox | Interior, manufacturer standard. | | Cost $ 195 | | | Deduct $ | |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **PART II (cont.)** |
|  | **State Price Quote Specification**  **DISTRICT-SUPPORTED OPTIONS**  **TYPE A**  **Use this document to bid both non-lift and lift, gas, diesel and propane buses.** | Vendor: Northwest Bus Sales  Mfr.: Starcraft |
|  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  | | |
| **ITEM** | Vendor must meet or exceed these specifications.  Item bid shall be specified in column to right. | | **VENDOR SPECIFICALLY IDENTIFY ITEM BID**  Price of items bid will establish the district cost. | |
| Video Camera Systems—Installed | Digital audio/video system for monitoring the passenger compartment with more than two cameras. | | Mfr. Rosco | |
| Model No. DVXC-4 | |
| Cost $ 1500 How many cameras 3 | |
| Video Camera Systems—Stop Sign Camera—Installed | Must meet state specification. | | ***Stand Alone System*** | ***Added to Interior System*** |
| Mfr. AngelTrax | Mfr. AngelTrax |
| Model No. Hybrid Quest | Model No. Hybrid Quest |
| Cost $ 2940 | Cost $ 3425 |
| How many cameras 1 | How many cameras 4 |
| Warning Light Monitor | 16 light monitoring system. | | ***Incandescent*** | ***LED Lights*** |
| Cost $ 625 | Cost $ 625 |
| Additional Wheelchair/Occupant Tie-down System—Installed | Must meet state specification. | | Mfr. Q’straint | |
| Model No. Q8101 / Q8-6326-A1 | |
| Cost per station $ 525 | |
| Windows | Laminated passenger-compartment side or rear glass. | | Side Cost $ 1100 | |
| Rear Cost $ 475 | |
| Both Cost $ 1575 | |
| Windows | Tinted. | | Cost $ STD | |